–	Bitstream file name: 
CC_ALF_CLIP_Sharp_1.bit

–	Explanation of bitstream features
This bitstream relates to enabling CC-ALF with filters that would exceed the output dynamic range and require a clip.

–	Profile, tier, and level for the bitstream
The bitstream is conformant with the Main 10 profile, Main tier, Level 4.1.

–	Max picture width and height, and any additional picture width and height values used (i.e., for reference picture resample or scalability) 
10-bit depth YUV420 pictures with luma resolution of 1920x1080. 
 
–	Picture rate 
60 frames per second

–	VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
The bitstream could be decoded using VVC software, tagged "VTM-8.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 

–	VTM release version number used to generate the bitstream, if applicable
The bitstream was encoded using modified VVC software, tagged "VTM-8.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 
The bitstream was encoded in random access configuration.
Gop size was 16, 33 frames were encoded.
Input sequence was BQTerrace_1920x1080_60.yuv, 1920x1080 resolution.

–	Contact name and email
Kiran Misra
misrak@sharplabs.com













Contact info:


