Bitstream  : LOSSLESS_A_HHI_1.bit
Resolution : 416x240 samples
Format     : 4:2:0 progressive
Profile    : auto
Tier       : Main Tier
Frame Rate : 60 Hz
Level      : 2.1
Bit Depth  : 8
Encoder    : VTM-8.0

Description:
The bitstream was generated by using an encoder operation mode leading to reconstruction samples that are exactly as the same as the input samples.

Contact Info:
Tung Nguyen
tung.nguyen@hhi.fraunhofer.de
