PDPC_A_Qualcomm_1.bit

This document is a description of the bitstream conformance test of luma PDPC.

Explanation of bitstream features:

The purpose of this test is to check if the clipping function in PDPC works well. Since the clipping is always applied when the block is predicted using intra horizontal or vertical mode, in this test each picture is a single I-slice where all the luma blocks are encoded using eithe horizontal or vertical intra prediction mode.

The bitstream could be decoded using VVC software, tagged "VTM-8.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 

Profile, tier, and level for the bitstream:
The bitstream is conformant with the Main 10 profile, Main tier, Level 3.1. The stream is coded as a 10-bit stream.

Max picture width and height and picture rate:
8-bit depth YUV420 pictures with luma resolution of 832x480. Picture rate is specified as 50 frames per second.

Contact info:
Luong Pham Van
Lphamvan@qti.qualcomm.com
Geert Van Der Auwera
geertv@qti.qualcomm.com