PDPC_B_Qualcomm_1.bit

This document is a description of the bitstream conformance test of luma PDPC.

Explanation of bitstream features:

The purpose of this test is to check if the functionality of PDPC works well for any block sizes. Since the PDPC modifies the prediction of intra blocks in any luma sizes and the modification weight is position dependent, testing the PDPC in every psibile size of luma is necessary.
Therefore, in this test, two constraints are added in the encoder side: 1) every CU in a frame (except the CUs within the border CTUs) is encoded using the samze square size (NxN), and 2) The fixed size NxN of a frame is POC dependent as N = 2^(POC%5 +2), so that N can vary from 4 to 64.
The number of encoded frames are 100 in all intra configuration with Dual-tree and ISP are set equal to 0.

The bitstream could be decoded using VVC software, tagged "VTM-8.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 

Profile, tier, and level for the bitstream:
The bitstream is conformant with the Main 10 profile, Main tier, Level 3.1. The stream is coded as a 10-bit stream with the following commandline:
 .\EncoderApp.exe -c encoder_intra_vtm_80.cfg -c BasketballDrill.cfg -f 100 -ip 1 -q 32 -ts 1 -c dummy.cfg -b PDPC_B_Qualcomm_1.bin -o rec.yuv -fs 0

Max picture width and height and picture rate:
8-bit depth YUV420 pictures with luma resolution of 832x480. Picture rate is specified as 50 frames per second.

Contact info:
Luong Pham Van
Lphamvan@qti.qualcomm.com
Geert Van Der Auwera
geertv@qti.qualcomm.com