- Bitstream file name
CUBEMAP_B_MediaTek_2

- Explanation of bitstream features
Pictures packed in the cubemap projection format with padding (size = 8 pixels) on the discontinuous edges and boundaries.
Generalized cubemap projection SEI message is sent in the bitstream with the following settings.

gcmp_packing_type         : 3 (6 columns x 1 rows)
gcmp_face_index           : 5 0 4 3 1 2
gcmp_face_rotation        : 0 0 0 0 0 0
gcmp_mapping_function_type: 1 (equi-angular mapping function)
gcmp_guard_band_flag      : 1
  gcmp_guard_band_type                   : 3
  gcmp_guard_band_boundary_exterior_flag : 1
  gcmp_guard_band_samples_minus1         : 7

- Profile, tier, and level for the bitstream
Main 10 profile
Main tier
Level 5

- Max picture width and height
5792x976

- Picture rate
30

- VTM decoder release version number able to correctly decode the bitstream with identical output
VTM-9.0tag (https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM)

- VTM release version number used to generate the bitstream
VTM-9.0tag (https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM)

- Encoder command line
./EncoderAppStatic -c CUBEMAP_B_MediaTek_2.cfg -b CUBEMAP_B_MediaTek_2.bit --SEIDecodedPictureHash=1 -ip 32 -f 60 -fs 0 -q 32 -o CUBEMAP_B_MediaTek_2.yuv

- Contact name and email of bitstream submitter
Ya-Hsuan Lee, louise.lee@mediatek.com