- Bitstream file name
VIRTUAL_B_MediaTek_2

- Explanation of bitstream features
Virtual boundaries signaled in PH are enabled only for the pictures with an odd POC value.
2 vertical virtual boundaries (x = 960, 1920) and 1 horizontal virtual boundaries (y = 960) are applied.

- Profile, tier, and level for the bitstream
Main 10 profile
Main tier
Level 5

- Max picture width and height
2880x1920

- Picture rate
30

- VTM decoder release version number able to correctly decode the bitstream with identical output
VTM-9.0tag (https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM)

- VTM release version number used to generate the bitstream
VTM-9.0tag (https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM) + encoder modification for turning on/off virtual boundaries for each picture

- Encoder command line
./EncoderAppStatic -c VIRTUAL_B_MediaTek_2.cfg -b VIRTUAL_B_MediaTek_2.bit --SEIDecodedPictureHash=1 -ip 32 -f 60 -fs 0 -q 37 -o VIRTUAL_B_MediaTek_2.yuv

- Contact name and email of bitstream submitter
Ya-Hsuan Lee, louise.lee@mediatek.com