–	Bitstream file name
16b444SPrlscp_A_2

–	Explanation of bitstream features
The purpose of this bitstream is to check that the decoder can properly decode slices with RLSCP enabled. The bitstream contains a single picture in 16-bit 4:4:4, VVCv1 tools set is enabled and VVCv2 tools are enabled. 
The picture is coded from "CrowdRun_1920x1080_50_16bit_444.rgb".  "cfg\partitioning\rect_slice_fixed_size.cfg" is used to set multiple slices in one picture. A modified VTM16.0 encoder is used. In the slices with even_numbered index, "sh_reverse_last_sig_coeff_flag" is set equal to 1. In the slices with odd_numbered index, "sh_reverse_last_sig_coeff_flag" is set equal to 0.

–	Profile, tier, and level for the bitstream
Profile: Main 16 4:4:4 still picture, tier: 0, level: 4.1

–	Max picture width and height, and any additional picture width and height values used (i.e., for reference picture resample or scalability)  
1920x1080

–	Picture rate 
50

–	VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
VTM16.0. The output is "GBR".

–	Contact name and email of bitstream submitter
Fan Wang
