16b444vvc1_A_2

This document is a description of the bitstream conformance test of vvcv1tool for main_16_444 profile.

Explanation of bitstream features:

Each picture is encoded as RA configuration.  

The bitstream could be decoded using VVC software, tagged "VTM-16.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 


Profile, and level for the bitstream:
The bitstream is conformant with the main_16_444 profile, Level 4.1.

Max picture width and height and picture rate:
16-bit depth RGB pictures with resolution of 1920x1080. 

Contact info:
Ru-Ling Liao
 