bitstream file : IP_B_1.bit
picture format : YUV 420
picture size   : 1920x1080 luma samples
picture rate   : 50 Hz
profile        : Main 10
tier           : Main Tier
level          : 4.1
decoder        : VTM-10.0
encoder        : VTM-10.0 (modified)
description    : 
  Forcing usage of all intra prediction modes
  favoring non-square blocks in encoder selection
contact info   : Pekka Astola 
                 Jani Lainema 
