test.264                 ........H.26L coded bitstream
test_dec.yuv             ........Output file, YUV 4:2:0 format
H:\Uncompressed\176x144\mobile_qcif.yuv             ........Ref sequence (for SNR)
10                       ........Decoded Picture Buffer size
0                        ........NAL mode (0=Annex B, 1: RTP packets)
500000                   ........Rate_Decoder
104000                   ........B_decoder
73000                    ........F_decoder
leakybucketparam.cfg     ........LeakyBucket Params

This is a file containing input parameters to the JVT H.264/AVC decoder.
The text line following each parameter is discarded by the decoder.
