Bitsteam Name					:PPCV444I5_Mitsubishi_A
Profile							:CAVLC 4:4:4 Intra
Entropy Coding					:CAVLC
Category						:CAVLC 4:4:4 14bit Intra

Number of Frames				:30
Source Width					:1920
Source Height					:1080

profile_idc						:44
level_idc						:41

constraint_set0_flag			:0
constraint_set1_flag			:0
constraint_set2_flag			:0
constraint_set3_flag			:1

chroma_format_idc				:3
bit_depth_luma_minus8			:6
bit_depth_chroma_minus8			:6
separate_colour_plane_flag		:1

Transform size					:8x8 and 4x4
seq_scaling_matrix_present_flag	:1
pic_scaling_matrix_present_flag	:0

MB Delta QP						:0

Slices per Picture				:4

POC type						:0

Loop Filter Parameters Flag		:0

Entropy Coding mode				:0

direct_spacial_mv_pred_flag		:None
direct_8x8_inference_flag		:None
Stored B picture				:None

Number of Reference Frames		:0

Frame Pictures					:1
Field Pictures					:0
mb_adaptive_frame_field_flag	:0

VUI								:None
SEI								:None
HRD Parameters					:None

IDR								:ALL Frames

Comments						:IIII, Q-matrix Loaded, deblocking, CAVLC, 4:4:4, 14bit

Volunteer to Generate			:Mitsubishi
Verification					:JM
Sequence						:card
