Stream Name:             PPH10I1_Panasonic_A.264
Stream Source:           PANASONIC
Video Sequence:          CrowdRun
Video Resolution:        1280x720 - 4:2:0  
Video Frames:            10
Frame/Field Coding:      Frame
Entropy Coding:          CAVLC
Slice Types:             IDR only
I Period:                1
Slices per Picture:      4
Number Ref Frames:       0
Constrained Intra Pred:  Off (Unconstrained)
Loop Filter:             On
SEI:                     No
VUI:                     No
Number Slice Groups:     1
Arbitrary Slice Order:   No
Redundant Slices:        No
Bit Depth Luma:          10
Bit Depth Chroma:        10
Transform 8x8 mode:      adaptive
Scaling Matrix:          No
