Annex 2 to AVC-743R

DSM-CC over ATM Architectures and Session Descriptions

This annex reproduces three architectures and the two session implementation descriptions in AVC-730 for future reference.

Figure 1: Hybrid ATM/MPEG switching of MPEG TS architecture

Figure 2: Session make-up in architecture 1

Figure 3: Full ATM switching of MPEG TS  with segregated session signaling

Figure 4: Full ATM switching of MPEG TS with integrated session signaling

Figure 5:  Session make-up in architectures 2 and 3

Reference

AVC-730 	"DSM-CC over ATM Architectures and Session Descriptions (BNR)", Janury 1995.

END