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1. Introduction


The aim of this contribution is to clarify the usage of the B-LLI message


in an H.310 terminal and to propose a document for an H.310 Implementors


Guide.


2. Problems to be solved


When a terminal has multiple protocol parameters, it can send multiple B-LLI


information elements to the called terminal in the Q.2931 SETUP message at


a call establish stage. A description of this procedure is needed.





For example, following situation may occur:


If a terminal has the two protocol suites such as H.310 ROT with TS stream and


H.310 ROT with PS stream, there is no appropriate B-LLI information element. Hence, a procedure is needed where ROT with TS B-LLI information element and ROT with PS B-LLI information element are sent to a called terminal and the called terminal chooses the preferred protocol suite from them.


3. Definition in Q.2931


Q.2931 Annex C defines the procedure for sending multiple B-LLI information element.


Up to three B-LLI information element may be included in a SETUP message.


The first B-LLI information element in the message is preceded by the Broadband repeat indicator information element in the case of multiple B-LLI information element transport.


The called terminal indicates a single choice from among the options offered in the SETUP messages by including the B-LLI  information element in the CONNECT message.


4. Proposed text for Implementors Guide


When the calling terminal has multiple protocol parameters and they cannot be expressed by a single B-LLI information element, the calling terminal shall send multiple B-LLI information elements according to Q.2931 Annex C. The procedure for choosing the B-LLI parameter at the called terminal is outside the scope of this implementors guide.





An example of the above case is where an H.310 terminal has both ROT with TS stream and ROT with PS stream capabilities. In this case, the calling terminal shall send B-LLI parameters both for ROT with TS stream and for ROT with PS stream in the preferred order included in the Q.2931 SETUP message. The called terminal shall choose one B-LLI information element and send it to the calling terminal in the CONNECT message.
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