purpose: Check that the decoder can properly decode bitstream if VSP is utilized.
conformance:    3DV-ATMv9.0
Level:          5.1
resolution:     1920x1080 (texture:depth=1:0.5)
# of views:     3+3
# of frames:    17
Coding Structure(time): IBP
Coding Structure(view): IP
Provider:       MERL

Shark QP31
