Sequence: Balloons
Resolution: 1024x768
Number of frames coded: 19
Temporal prediction structure: IBP
Interview prediction structure: PIP
Profile idc specified in bitstream: 139
Leve idc specified in bitstream: 5.1
Frame rate: 30Hz
Purpose: texture first coding order enabled, DoNBDV disparity derivation method is utilized for coding of texture components of dependent views
Bitstream name: MVDCT-7
