* Bitstream file name
  - ENTROPY_A_Chipsnmedia_2.bit

* Explanation of bitstream features
  - This bitstream provides a high bitrate example (the average bitrate across the bitstream is 43.5Mbps) conformant to Main10 profile, Main Tier and Level 5.1.
  - This bitstream is encoded using 'ParkRunning3' sequence
  - low delay P with intra preiod 8
  - MIP on
  - Total 60 frames

* Profile, tier, and level for the bitstream
  - main10 profile, main tier, level 5.1

* Max picture width and height, and any additional picture width and height values used
  - 3840x2160

* Picture rate
  - 60

* VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
  - The bitstream could be decoded using VVC software, tagged VTM-10.2 in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM.

* VTM release version number used to generate the bitstream, if applicable
  - VVC software, tagged VTM-10.2 in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM.

* Contact name and email
  - M.-W. Kim (bentley.kim@chipsnmedia.com)
  - D.-Y. Kim (brad.kim@chipsnmedia.com)
