
bitstream file : JCCR_D_HHI_3.bit
picture format : YUV 420
picture size   : 1920x1080 luma samples
picture rate   : 24 Hz
profile        : Main 10
tier           : Main Tier
level          : 4
decoder        : VTM-10.0
encoder        : modified VTM-10.0

description    :
This bitstream exercises joint chroma residual coding in combination with other tools.
The bitstream consists of two coded video sequences with the folloiwng properties:
- The first CVS uses a random selection of the jointCbCr sign flag, forces the usage of all possible jointCbCr modes, non-related features (inter tools, ALF, ...) are disabled, MTS, LFNST, LMCS, and DepQuant are disabled.
- The first CVS uses a random selection of the jointCbCr sign flag, forces the usage of all possible jointCbCr modes, non-related features (inter tools, ALF, ...) are disabled, MTS (for intra), LFNST, LMCS, and DepQuant are enabled.

contact info   : Heiko Schwarz (heiko.schwarz@hhi.fraunhofer.de)
