Bitstream file name: CUBEMAP_B_MediaTek_3.bit
Conformance point:   VTM-10.0
Resolution:          5792x976
Format:              4:2:0
Frame rate:          30 frames/sec
Profile:             Main 10 profile
Tier:                Main tier
Level:               5

Decoded with VTM Tag: VTM-10.0 (45dfe068)
Encoded with VTM Tag: VTM-10.0 (45dfe068)
Encoder command line:
./EncoderAppStatic -c CUBEMAP_B_MediaTek_3.cfg -b CUBEMAP_B_MediaTek_3.bit --SEIDecodedPictureHash=1 -ip 32 -f 60 -fs 0 -q 32 -o CUBEMAP_B_MediaTek_3.yuv

Bitstream feature:
Pictures packed in the cubemap projection format with padding (size = 8 pixels) on the discontinuous edges and boundaries.
Generalized cubemap projection SEI message is sent in the bitstream with the following settings.
gcmp_packing_type         : 3 (6 columns x 1 rows)
gcmp_face_index           : 5 0 4 3 1 2
gcmp_face_rotation        : 0 0 0 0 0 0
gcmp_mapping_function_type: 1 (equi-angular mapping function)
gcmp_guard_band_flag      : 1
  gcmp_guard_band_type                   : 3
  gcmp_guard_band_boundary_exterior_flag : 1
  gcmp_guard_band_samples_minus1         : 7


Contact info:
Ya-Hsuan Lee, louise.lee@mediatek.com