Bitstream file name: CUBEMAP_C_MediaTek_3.bit
Conformance point:   VTM-10.0
Resolution:          3872x1280
Format:              4:2:0
Frame rate:          30 frames/sec
Profile:             Main 10 profile
Tier:                Main tier
Level:               5

Decoded with VTM Tag: VTM-10.0 (45dfe068)
Encoded with VTM Tag: VTM-10.0 (45dfe068)
Encoder command line:
./EncoderAppStatic -c CUBEMAP_C_MediaTek_3.cfg -b CUBEMAP_C_MediaTek_3.bit --SEIDecodedPictureHash=1 -ip 32 -f 60 -fs 0 -q 32 -o CUBEMAP_C_MediaTek_3.yuv

Bitstream feature:
Pictures packed in the hemisphere cubemap projection format with padding (size = 16 pixels) on the discontinuous edges.
Generalized cubemap projection SEI message is sent in the bitstream with the following settings.
gcmp_packing_type         : 4 (5 columns x 1 rows)
gcmp_face_index           : 3 5 0 4 2
gcmp_face_rotation        : 2 0 0 0 2
gcmp_mapping_function_type: 0 (conventional cubemap)
gcmp_guard_band_flag      : 1
  gcmp_guard_band_type                   : 1
  gcmp_guard_band_boundary_exterior_flag : 0
  gcmp_guard_band_samples_minus1         : 15


Contact info:
Ya-Hsuan Lee, louise.lee@mediatek.com