* Bitstream file name
  - MPM_A_LGE_3.bit
* Explanation of bitstream features
  - Enable all conditions to generate MPM candidate for all the sizes of the blocks, i.e. all WxH-sized TUs, where both W and H are equal to one of the following values: {4, 8, 16 or 32}
  - Enable all intra coding tools except MIP
  - Bitstream for ¡°Tango2¡± test sequence of ClassA1 with QP 37
* Profile, tier, and level for the bitstream
  - Main 10 profile, Main tier, and Level 5.1
* Max picture width and height, and any additional picture width and height values used (i.e., for reference picture resample or scalability)  
  - Max picture width: 3840 and Max picture height: 2160
* Picture rate 
  - Picture rate: 60
* VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
  - The bitstream could be decoded using VVC software, tagged ¡°VTM-10.0¡± in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM.
* VTM release version number used to generate the bitstream, if applicable
  - VVC software, tagged ¡°VTM-10.0¡± in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM.
  - The bitstream was encoded in intra configuration.
* Contact name and email
  - Jin Heo (jin78.heo@lge.com) 
