Bitstream file name: CUBEMAP_A_MediaTek_3.bit
Conformance point:   VTM-10.0
Resolution:          2880x1920
Format:              4:2:0
Frame rate:          30 frames/sec
Profile:             Main 10 profile
Tier:                Main tier
Level:               5

Decoded with VTM Tag: VTM-10.0 (45dfe068)
Encoded with VTM Tag: VTM-10.0 (45dfe068)
Encoder command line:
./EncoderAppStatic -c CUBEMAP_A_MediaTek_3.cfg -b CUBEMAP_A_MediaTek_3.bit --SEIDecodedPictureHash=1 -ip 32 -f 60 -fs 0 -q 37 -o CUBEMAP_A_MediaTek_3.yuv

Bitstream feature:
Pictures packed in the cubemap projection format without padding.
Generalized cubemap projection SEI message is sent in the bitstream with the following settings.
gcmp_packing_type         : 2 (3 columns x 2 rows)
gcmp_face_index           : 5 0 4 3 1 2
gcmp_face_rotation        : 0 0 0 0 0 0
gcmp_mapping_function_type: 2 (coefficients and affected flags as follows)
  gcmp_function_coeff_u             : 0.28 0.28 0.28 0.28 0.4 0.28
  gcmp_function_u_affected_by_v_flag: 0 0 0 0 1 0
  gcmp_function_coeff_v             : 0.4 0.4 0.4 0.28 0.28 0.28
  gcmp_function_v_affected_by_u_flag: 1 1 1 0 0 0
gcmp_guard_band_flag      : 0


Contact info:
Ya-Hsuan Lee, louise.lee@mediatek.com