–	Bitstream file name: 
	QUANT_C_Huawei_2.bit

–	Explanation of bitstream features
	DBF with transform skip (CTC DBF parameters). Due to low QP DBF is not actually used. 

–	Profile, tier, and level for the bitstream
	The bitstream is conformant with the Main 10 profile, Main tier, Level 4

–	Max picture width and height, and any additional picture width and height values used (i.e., for reference picture resample or scalability) 
	8-bit depth YUV420 input pictures with luma resolution of 1280x720
	
–	Picture rate 
	60 frames per second

–	VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
	Decoder : VTM-10.0 

–	VTM release version number used to generate the bitstream, if applicable
	Encoder : VTM-10.0 modified in order to allow DBF together with lossless configuration (Transform and Quantization are skipped) 
	Configuration: RandomAccess
	Gop size : 16
	Number of frames encoded : 3
	Input sequence: Johnny_1280x720_60.yuv
	Resolution: 1280x720
	Encoder command line:
		-c "..\..\..\..\cfg\per-sequence\Johnny.cfg" -i "Johnny_1280x720_60.yuv" -c "..\..\..\..\cfg\encoder_randomaccess_vtm.cfg" -c QUANT_C_Huawei_2_lossless.cfg -wdt 1280 -hgt 720 -f 3  -b QUANT_C_Huawei_2.bit -o rec.yuv -dph 1  

–	Contact name and email
	Chernyak Roman (chernyak.roman@huawei.com)
