Bitfile:             ENT444HIGHTIER_D_Sony_3.bit
Profile:             main_10_444
Level:               5.1
Tier:                high
Image size:          4096 x 2176
Bit depth:           10
Chroma format:       4:4:4 (YCbCr)
Frame rate:          60P
VCL Bits per frame:  6666664
Created with:        Modified VTM10.0 encoder
Decoded with:        VTM10.0 decoder
Contact:             Karl Sharman (karl.sharman@sony.com)

Content description:
  The bit-stream contains 3 independent sequences containing one picture, formed from one slice.
  Each sequence contains the maximum number of bits, given the profile, level and tier, and assuming equal distribution
   of bits between pictures coded at the maximum pixel rate for the level.
  The 3 concatenated sequences are as follows:
    1/ the first picture does not require any CABAC zero words,
    2/ the second picture requires one CABAC zero word,
    3/ the third picture requires a substantial quantity of CABAC zero words (71% of the bit-stream is padding).
    All 3 pictures have a very low subjective quality level due to the artificial nature of these bit-streams.
  All VCL NAL units contain almost (within 3 bytes worth) of the maximum number of allowed bins, for their size.
Note when running VTM10.0, the decoder checks the next VCL NALU before completing the current VCL NALU.
  This means that CABAC zero words are reported twice - once for the current slice/picture and the next slice/picture.
