Bitstream file name: VIRTUAL_B_MediaTek_3.bit
Conformance point:   VTM-10.2
Resolution:          2880x1920
Format:              4:2:0
Frame rate:          30 frames/sec
Profile:             Main 10 profile
Tier:                Main tier
Level:               5

Decoded with VTM Tag: VTM-10.2 (7abf654d)
Encoded with VTM Tag: VTM-10.2 (7abf654d) + encoder modification for turning on/off virtual boundaries for each picture
Encoder command line:
./EncoderAppStatic -c VIRTUAL_B_MediaTek_3.cfg -b VIRTUAL_B_MediaTek_3.bit --SEIDecodedPictureHash=1 -ip 32 -f 60 -fs 0 -q 37 -o VIRTUAL_B_MediaTek_3.yuv

Bitstream feature:
Virtual boundaries signaled in PH are enabled only for the pictures with an odd POC value.
2 vertical virtual boundaries (x = 960, 1920) and 1 horizontal virtual boundaries (y = 960) are applied.


Contact info:
Ya-Hsuan Lee, louise.lee@mediatek.com