- Bitstream file name
CUBEMAP_A_MediaTek_1

- Explanation of bitstream features
Pictures packed in the cubemap projection format without padding.
Generalized cubemap projection SEI message is sent in the bitstream with the following settings.

gcmp_packing_type         : 2 (3 columns x 2 rows)
gcmp_face_index           : 5 0 4 3 1 2
gcmp_face_rotation        : 0 0 0 0 0 0
gcmp_mapping_function_type: 2 (coefficients and affected flags as follows)
  gcmp_function_coeff_u             : 0.28 0.28 0.28 0.28 0.4 0.28
  gcmp_function_u_affected_by_v_flag: 0 0 0 0 1 0
  gcmp_function_coeff_v             : 0.4 0.4 0.4 0.28 0.28 0.28
  gcmp_function_v_affected_by_u_flag: 1 1 1 0 0 0
gcmp_guard_band_flag      : 0

- Profile, tier, and level for the bitstream
Main 10 profile
Main tier
Level 5.2

- Max picture width and height
2880x1920

- Picture rate
30

- VTM decoder release version number able to correctly decode the bitstream with identical output
VTM-8.0tag (837b7dfe)

- VTM release version number used to generate the bitstream
VTM-8.0tag (837b7dfe)

- Encoder command line
./EncoderAppStatic -c encoder_randomaccess_vtm.cfg -b CUBEMAP_A_MediaTek_1.bit --SEIDecodedPictureHash=1 -ip 32 -f 300 -fs 0 -q 37 -o CUBEMAP_A_MediaTek_1.yuv

- Contact name and email of bitstream submitter
Ya-Hsuan Lee, louise.lee@mediatek.com