- Bitstream file name
CUBEMAP_C_MediaTek_1

- Explanation of bitstream features
Pictures packed in the hemisphere cubemap projection format with padding (size = 16 pixels) on the discontinuous edges.
Generalized cubemap projection SEI message is sent in the bitstream with the following settings.

gcmp_packing_type         : 4 (5 columns x 1 rows)
gcmp_face_index           : 3 5 0 4 2
gcmp_face_rotation        : 2 0 0 0 2
gcmp_mapping_function_type: 0 (conventional cubemap)
gcmp_guard_band_flag      : 1
  gcmp_guard_band_boundary_type : 0
  gcmp_guard_band_samples_minus1: 15

- Profile, tier, and level for the bitstream
Main 10 profile
Main tier
Level 5.2

- Max picture width and height
3872x1280

- Picture rate
30

- VTM decoder release version number able to correctly decode the bitstream with identical output
VTM-8.0tag (837b7dfe)

- VTM release version number used to generate the bitstream
VTM-8.0tag (837b7dfe)

- Encoder command line
./EncoderAppStatic -c encoder_randomaccess_vtm.cfg -b CUBEMAP_C_MediaTek_1.bit --SEIDecodedPictureHash=1 -ip 32 -f 300 -fs 0 -q 32 -o CUBEMAP_C_MediaTek_1.yuv

- Contact name and email of bitstream submitter
Ya-Hsuan Lee, louise.lee@mediatek.com