
bitstream file : DQ_D_HHI_1.bit
picture format : YUV 420
picture size   : 1920x1080 luma samples
picture rate   : 24 Hz
profile        : Main 10
tier           : Main Tier
level          : 4
decoder        : VTM-8.0
encoder        : VTM-8.0

description    :
 - enable dependent quantization for all pictures
 - disable non-related features (inter tools, ALF, ...)
 - disable MTS
 - disable LFNST

contact info   : Heiko Schwarz (heiko.schwarz@hhi.fraunhofer.de)

