
bitstream file : JCCR_C_HHI_1.bit
picture format : YUV 420
picture size   : 1920x1080 luma samples
picture rate   : 24 Hz
profile        : Main 10
tier           : Main Tier
level          : 4
decoder        : VTM-8.0
encoder        : modified VTM-8.0

description    :
 - random selection of jointCbCr sign flag: force usage of all possible jointCbCr modes
 - disable non-related features (inter tools, ALF, ...)
 - disable MTS, LFNST, LMCS, and DepQuant

contact info   : Heiko Schwarz (heiko.schwarz@hhi.fraunhofer.de)

