–	Bitstream file name
MERGE_A4_Qualcomm_1


–	Explanation of bitstream features
Maximum number of merge candidate (MaxNumMergeCand) = 4 and Maximum number of GMO merge candidate (MaxNumGpmMergeCand ) = 4


–	Profile, tier, and level for the bitstream
Main10 profile
Main tier
Level 5.1


–	Max picture width and height, and any additional picture width and height values used (i.e., for reference picture resample or scalability)  
width = 3840
height = 2160

–	Picture rate 
frame rate = 60


–	VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
VTM8

–	VTM release version number used to generate the bitstream, if applicable
VTM8

–	Contact name and email of bitstream submitter
Wei-Jung Chien, wchien@qti.qualcomm.com