PALETTE_B_Alibaba_1.bit

This document is a description of the bitstream conformance test of Palette modes.

Explanation of bitstream features:

Each picture is a single I-slice. The bit-stream of generated in such a way that majority of the coding unit is coded using palette mode. 

The bitstream could be decoded using VVC software, tagged "VTM-8.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 

The bitstream was encoded in All intra configuration. The reason of using intra-only configuration becasue the possibility of palette mode in I slice is relatively higher than P and B slice. 

Profile, tier, and level for the bitstream:
The bitstream is conformant with the 444 profile, Main tier, Level 6.

Max picture width and height and picture rate:
8-bit depth YUV444 pictures with luma resolution of 1920x1080. Picture rate is specified as 60 frames per second.

Contact info:
Mohammed sarwer
m.sarwer@alibaba-inc.com 

