- Bitstream file name
VIRTUAL_B_MediaTek_1

- Explanation of bitstream features
Virtual boundaries signalled in PH are disabled and enabled alternately in decoding order.
2 vertical virtual boundaries (x = 960, 1920) and 1 horizontal virtual boundaries (y = 960) are applied.

- Profile, tier, and level for the bitstream
Main 10 profile
Main tier
Level 5.2

- Max picture width and height
2880x1920

- Picture rate
30

- VTM decoder release version number able to correctly decode the bitstream with identical output
VTM-8.0tag (837b7dfe)

- VTM release version number used to generate the bitstream
VTM-8.0tag (837b7dfe) + encoder modification for turning on/off virtual boundaries for each picture

- Contact name and email of bitstream submitter
Ya-Hsuan Lee, louise.lee@mediatek.com