- Bitstream file name
CUBEMAP_C_MediaTek_2

- Explanation of bitstream features
Pictures packed in the hemisphere cubemap projection format with padding (size = 16 pixels) on the discontinuous edges.
Generalized cubemap projection SEI message is sent in the bitstream with the following settings.

gcmp_packing_type         : 4 (5 columns x 1 rows)
gcmp_face_index           : 3 5 0 4 2
gcmp_face_rotation        : 2 0 0 0 2
gcmp_mapping_function_type: 0 (conventional cubemap)
gcmp_guard_band_flag      : 1
  gcmp_guard_band_type                   : 1
  gcmp_guard_band_boundary_exterior_flag : 0
  gcmp_guard_band_samples_minus1         : 15

- Profile, tier, and level for the bitstream
Main 10 profile
Main tier
Level 5

- Max picture width and height
3872x1280

- Picture rate
30

- VTM decoder release version number able to correctly decode the bitstream with identical output
VTM-9.0tag (https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM)

- VTM release version number used to generate the bitstream
VTM-9.0tag (https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM)

- Encoder command line
./EncoderAppStatic -c CUBEMAP_C_MediaTek_2.cfg -b CUBEMAP_C_MediaTek_2.bit --SEIDecodedPictureHash=1 -ip 32 -f 60 -fs 0 -q 32 -o CUBEMAP_C_MediaTek_2.yuv

- Contact name and email of bitstream submitter
Ya-Hsuan Lee, louise.lee@mediatek.com