Bitstream  : 12b444Ierrc_A_2.bit
Resolution : 1920x1080
Format     : 4:4:4 progressive
Profile    : Main 12 444 Intra
Tier       : Main Tier
Frame Rate : 24 fps
Level      : 6.2
Bit Depth  : 12
Encoder    : Modified VTM-16.0 (range of QPs)
Decoder    : VTM-16.0

Description:
12 bits video data with 4:4:4 chroma format is being coded in all intra configuraition, testing of the ERRC functionality, PRRC is enabled.

Contact Info:
Dmytro Rusanovskyy

