12b444Ivvc1_A_2.bit

This document is a description of the bitstream conformance test of vvcv1tool for main_12_444_intra profile.

Explanation of bitstream features:

Each picture is Encoded as AI configuration.  

The bitstream could be decoded using VVC software, tagged "VTM-16.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 


Profile, and level for the bitstream:
The bitstream is conformant with the main_12_444_intra profile, Level 4.1.

Max picture width and height and picture rate:
12-bit depth YUV444 pictures with luma resolution of 1920x1080. Picture rate is specified as 25 frames per second.

Contact info:
Mohammed sarwer
 

