PALETTE_E_2.bit

This document is a description of the bitstream conformance test of Palette modes.

Explanation of bitstream features:

Each picture is Encoded as RA configuration. The bit-stream of generated in such a way that majority of the coding unit is coded using palette mode. 

The bitstream could be decoded using VVC software, tagged "VTM-11.0" in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM. 

The bitstream was encoded in RA configuration. 

Profile, tier, and level for the bitstream:
The bitstream is conformant with the 444 profile, Main tier, Level 3.

Max picture width and height and picture rate:
8-bit depth YUV420 pictures with luma resolution of 1280x720. Picture rate is specified as 30 frames per second.

Contact info:
Mohammed sarwer
 

