Bitstream  : 12b444prrc_A_Qualcomm_1.bit
Resolution : 1920x1080
Format     : 4:4:4 progressive
Profile    : Main 12 444
Tier       : Main Tier
Frame Rate : 60 fps
Level      : 6.2
Bit Depth  : 12
Encoder    : VTM-14.0
Decoder    : VTM-14.0

Description:
12 bits video data with 4:4:4 chroma format is being coded with random access picture types, testing of the PRRC functionality, ERRC is enabled.

Contact Info:
Dmytro Rusanovskyy
dmytror@qti.qualcomm.com
