Bitstream  : 16b444Iprrc_A_Qualcomm_1.bit
Resolution : 1920x1080
Format     : 4:4:4 progressive
Profile    : Main 16 444 Intra
Tier       : Main Tier
Frame Rate : 50 fps
Level      : 6.2
Bit Depth  : 16
Encoder    : Modified VTM-14.0 (wide range of QPs)
Decoder    : VTM-14.0

Description:
16 bits RGB video data with is being coded with intra picture types testing of the PRRC functionality, ERRC is enabled.

Contact Info:
Dmytro Rusanovskyy
dmytror@qti.qualcomm.com
