* Bitstream file name
  - 12b444SPetsrc_E_1.bit
* Explanation of bitstream features
  - The bitstream is provided to verify the ETSRC tool
  - Slice level signal of the Rice parameter in TSRC
  - 12-bit YUV sequences "Market3Clip4000r2_1920x1080p_50_12b_pq_709_ct2020_444" with QP -13, all-intra configuration of 1 frames
* Profile, tier, and level for the bitstream
  - Main 12 4:4:4 Still Picture, main tier, level 6.2
* Max picture width and height
  - Max picture width and height are 1920 and 1080
* Picture rate 
  - Picture rate is 50
* VTM decoder release version number able to correctly decode the bitstream with identical output
  - The bitstream could be decoded using VVC software, tagged ¡§VTM-14.0¡¨ in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM
* VTM release version number used to generate the bitstream, if applicable
  - The bitstream is generated using VVC software, tagged ¡§VTM-14.0¡¨ in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM
* Contact name and email of bitstream submitter
  - Hong-Jheng Jhu (  )