Bitfile:       10b444P12_E_Sony_2.bit
Profile:       Main 12 444
Tier:          High
Level:         5.1
Image size:    3840x2160
Bit depth:     10
Chroma format: 444
Frame rate:    50P
Created by:    VTM15.2 plus GCI and other fixes (https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM/-/tree/8b91436e71c318d0c17c99eeabf28b5db4c8f058)
Decoded by:    VTM16.0
Contact:       Adrian Browne (adrian.browne@sony.com)

Content description:
               A random access sequence of 10-bit 444 data encoded in the Main 12 444 profile.
               VVCv2 tools (EPP, ERRC, PRRC, ETSRC, RLSCP) are not used due to bit depth constraint.
