Bitstream  : 12b444Ierrc_B_Qualcomm_2.bit
Resolution : 1920x1080
Format     : 4:4:4 progressive
Profile    : Main 12 444 Intra
Tier       : Main Tier
Frame Rate : 50 fps
Level      : 6.2
Bit Depth  : 12
Encoder    : Modified VTM-16.0 (range of QPs)
Decoder    : VTM-16.0

Description:
12 bits video data with 4:4:4 chroma format is being coded in all intra configuration, testing of the ERRC functionality, PRRC is disabled

Contact Info:
Dmytro Rusanovskyy
dmytror@qti.qualcomm.com
