–	Bitstream file name
16b444SPwpp_A_OPPO_1

–	Explanation of bitstream features
The purpose of this bitstream is to check that the decoder can properly decode slices with WPP enabled. The bitstream contains a single picture in 16-bit 4:4:4 chroma format, VVCv1 tools set is enabled and VVCv2 tools are enabled. 
The pictures is coded from "ParkJoy_1920x1080_50_16bit_444.rgb" with WPP enable. "cfg\partitioning\rec_slice_fixed_size.cfg" is used to set multiple slices in one picture.

–	Profile, tier, and level for the bitstream
Profile: Main_16_4:4:4_still_picture, tier: 0, level: 4.1

–	Max picture width and height, and any additional picture width and height values used (i.e., for reference picture resample or scalability)  
1920x1080

–	Picture rate 
50

–	VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
VTM16.0

–	Contact name and email of bitstream submitter
Zhihuang Xie
xiezhihuang@oppo.com