Bitstream  : 16b444errc_C_Qualcomm_2.bit
Resolution : 1920x1080
Format     : 4:4:4 progressive
Profile    : Main 16 444
Tier       : Main Tier
Level      : 6.2
Frame Rate : 50 fps
Bit Depth  : 16
Encoder    : Modified VTM-16.0 (wide range of QPs)
Decoder    : VTM-16.0, decoded with run time parameter --OutputColourSpaceConvert=GBRtoRGB

Description:
16 bits RGB video data with is being coded with random access picture types, testing of the ERRC functionality, PRRC is enabled.

Contact Info:
Dmytro Rusanovskyy
dmytror@qti.qualcomm.com
