Stream Name:  CVSE3_Sony_H
Stream Source:  Sony  
Video Sequence:  Foreman  
Video Resolution:  QCIF  
Video Frames:  278  
Frame/Field Coding:  Frame  
Entropy Coding:  CAVLC  
Slice Types:  IPB
I Period:  0  
Slices per Picture:  1  
Conformance Point:  JVT-G050r1 (2003/6/02)  

POC Type:  0  
Number Reference Frames:  4  
IDR:  First frame  
Ref Pic List Reordering:  No  
Adaptive Ref Pic Marking Mode:  Off  
Constrained Intra Prediction:  Off (Unconstrained)  
Weighted Prediction (P):  Off  
Weighted Biprediction (B):  Off  
Direct Prediction:  Temporal  
Direct 8x8 Inference:  On  
Loop Filter:  On  
SEI:  Yes (buffering_period, pic_timing with pic_struct)
VUI:  Yes  
Number Slice Groups: 1
Long-term Ref Frames: No
MMCO: No
Arbitrary Slice Order: No
Redundant Slices: No

3:2 pull-down (24fps -> 29.97 fps)
347 output frames
CVSE3_Sony_G-norpt.yuv is decoded output
CVSE3_Sony_G.yuv has field repeat defined by pic_struct