Bitstream                           MPS_MW_A
Bitstream source                    Mcubeworks Inc.
Conformance Point                   JVT-G050r1
Video Sequence                      Foreman
Profile                             Baseline
Entropy coding                      CAVLC
Video Coded num. of frames          150
Video Resolution/FPS                QCIF / 15fps
Intra period                        30 ( = 2 sec.)
POC Type                            0
Loop filter                         ON
Direct Prediction                   NO
Direct 8x8 Inference                OFF
Weighted Pred (P)                   OFF
Weighted Bipred (B)                 OFF
Num. of ref-frames                  3
Ref Pic List Reorder                NO
MMCO                                NO
Long-term Ref Frames                NO
Number Slice Groups                 1
Picture structure                   Frame only
VUI                                 NO
SEI                                 NO
Slice type                          IPPIPP...
Slice structure                     1 slice / picture
Constrained intra                   OFF
IDR                                 all-I
Arbitrary Slice Order               NO
Redundant Slices                    NO

Number of PPS                       2
