FRExt Conformance Bitstream
#FREH10-1
10-Bit High 4:2:0
Bitsream Specification

Specification:  All slices are coded as I, P or B Slices.  Each Picture contains only one slice.  Disable_deblocking_Filter_idc_is equal to 1, specifiying disabling of the deblocking filter process.  Entropy_coding_mode_flag is equal to 0, specifying the CAVLC parsing process.  Pic_order_count_type is equal to 0.  Frame_mbs_only_flag is equal to 1.  Chroma_format_idc is equal to 1.  Both bit_depth_luma_minus8 and bit_depth_chroma_minus8 are set equal to 2.  All NAL units are encapsulated into the byte stream format specified in Annex B in ITU-T Rec.H.264|ISO/IEC 14496-10.
Functional Stage:  Decoding of I, P, and B Slices for 4:2:0 10-bit content
Purpose:  Check that the decoder can properly decode I, P, and B slices for 4:2:0 10-bit.