Volunteer                                          Vidyo
Description                                        MT-4 + slice_skip_flag
Scalability Type                                   MGS/Temporal     
Bitstream                                          SVCBMT-10 
Bitstream Number                                   0    
Width                                              352  
Height                                             240  
Frame rate                                         30.00
Number of frames                                   200  
chroma_format_idc                                  -    
bit_depth_luma_minus8                              -    
bit_depth_chroma_minus8                            -    
residual_color_transform_flag                      -    
separate_colour_plane_flag                         -    
profile_idc                                        66   
level_idc                                          13   
constraint_set0_flag                               1    
constraint_set1_flag                               1    
constraint_set2_flag                               1    
constraint_set3_flag                               0    
Number of IDR access units                         1    
Number of slices per picture                       >1    
seq_scaling_matrix_present_flag                    -    
transform_8x8_mode_flag                            -    
pic_scaling_matrix_present_flag                    -    
qpprime_y_zero_transform_bypass_flag               -    
slice_qp_delta == 0                                0    
mb_qp_delta == 0                                   0    
chroma_qp_index_offset                             0    
frame_mbs_only_flag                                1    
mb_adaptive_frame_field_flag                       -    
field_pic_flag                                     -    
deblocking_filter_control_present_flag             1    
disable_deblocking_filter_idc                      2    
slice_alpha_c0_offset_div2                         !=0    
slice_beta_offset_div2                             !=0    
entropy_coding_mode_flag                           0    
I_PCM                                              -    
direct_spatial_mv_pred_flag                        -    
direct_8x8_inference_flag                          1    
weighted_pred_flag                                 0    
weighted_bipred_idc                                0    
num_ref_frames                                     4    
gaps_in_frame_num_value_allowed_flag               1    
ref_pic_list_reordering_flag                       1    
adaptive_ref_pic_marking_mode_flag                 1    
num_slice_groups_minus1                            0    
slice_group_map_type                               -    
pic_order_cnt_type                                 2    
frame_cropping_flag                                0    
VUI                                                -    
HRD                                                -    
SEI                                                0    
priority_id                                        0    
dependency_id                                      0    
quality_id                                         0    
ref_layer_dq_id                                    -1   
DependencyIdMax                                    0    
TemporalIdMax                                      3    
DQIdMax                                            0    
DependentDId                                            
Number of EIDR slices                              -    
extended_spatial_scalability                       -    
SpatialResolutionChangeFlag                        -    
chroma_phase_x_plus1_flag                          -    
chroma_phase_y_plus1                               -    
seq_ref_layer_chroma_phase_x_plus1_flag            -    
seq_ref_layer_chroma_phase_y_plus1                 -    
seq_scaled_ref_layer_left_offset                   -    
seq_scaled_ref_layer_top_offset                    -    
seq_scaled_ref_layer_right_offset                  -    
seq_scaled_ref_layer_bottom_offset                 -    
ref_layer_chroma_phase_x_plus1_flag                     
ref_layer_chroma_phase_y_plus1                          
constrained_intra_resampling_flag                  -    
no_inter_layer_pred_flag                           -    
use_ref_base_pic_flag                              0    
store_ref_base_pic_flag                            0    
output_flag                                        1    
discardable_flag                                   0    
slice_header_restriction_flag                      -    
scan_idx_start                                     -    
scan_idx_end                                       -    
seq_tcoeff_level_prediction_flag                   -    
adaptive_tcoeff_level_prediction_flag              -    
slice_skip_flag                                    -    
num_mbs_in_slice_minus1                            -    
adaptive_base_mode_flag                            -    
default_base_mode_flag                             -    
adaptive_motion_prediction_flag                    -    
default_motion_prediction_flag                     -    
adaptive_residual_prediction_flag                  -    
default_residual_prediction_flag                   -    
base_pred_weight_table_flag                        -    
inter_layer_deblocking_filter_control_present_flag -    
disable_inter_layer_deblocking_filter_idc          -    
inter_layer_slice_alpha_c0_offset_div2             -    
inter_layer_slice_beta_offset_div2                 -    
