This zip file contains material related to Q15-I-26.

Encoder configuration files:
   hall24.cfg
   fm48.cfg

Frame-specific PSNR values:
   *.psnr

File locations:
   Error-free PSNR reside in snr_hall and snr_fm.
   Nokia decoder PSNRs reside in nok_hall and nok_fm.
   TMN decoder PSNRs reside in tmn_hall and tmn_fm.

The file names have the following notation.

Encoding strategy:
   no       RTYPE is always zero and picture layer data is never repeated
   s        RTYPE is always zero and picture layer data is repeated if needed
   r        RTYPE is non-constant and picture layer data is never repeated
   rs       RTYPE is non-constant and picture layer data is repeated if needed

Error patterns:
   dect_10  DECT 1.4 km/h 10dB
   dect_20  DECT 1.4 km/h 20dB
   wcdma_3  wcdma-64kb-211hz-3
   wcdma_4  wcdma-64kb-211hz-4
