Files in the folder
CAMANL3_Sand_E_Readme.txt       This file
CAMANL3_Sand_E.264              Bitstream 
CAMANL3_Sand_E.yuv              Reconstructed YUV file
CAMANL3_Sand_E.trc              Decoder trace file
----------------------------------------------------------------------
Encoder configuration:
Stream Name:             CAMANL3_Sand_E
Stream Source:           Sand Video
Video Sequence:          Mobile  
Video Resolution:        CIF  
Video Frames:            30 
Frame/Field Coding:      MB Adaptive
Entropy Coding:          CABAC  
GOP Structure:           IDR B B P...
Slices per Picture:      1  
Conformance Point:       JVT-G050r1  
POC Type:                0  
Number Ref Frames:       4  
IDR:                     First frame  
Ref Pic List Reorder:    No  
Adapt Ref Pic Mark:      No
Constrained Intra Pred:  No
Weighted Pred (P):       No
Weighted Bipred (B):     No
Direct Prediction:       Temporal 
Direct 8x8 Inference:    On
Loop Filter:             No  
SEI:                     No  
VUI:                     No  
Number Slice Groups:     1
Long-term Ref Frames:    No
MMCO:                    No
Arbitrary Slice Order:   No
Redundant Slices:        No
