Bitstream source                    Mcubeworks Inc.
Bitstream                           MIDR_MW_D
Conformance Point                   JVT-G050r1
Profile                             Baseline
Video Sequence                      Foreman
Video Resolution/FPS                QCIF / 15fps
Video Coded num. of frames          100
Entropy coding                      CAVLC
Slice type                          IPPIPP...
Picture structure                   Frame only
Slice structure                     1 slice / picture
Intra period                        30 ( = 2 sec.)
POC Type                            0
Loop filter                         ON
Ref Pic List Reorder                NO
Adapt Ref Pic Mark                  OFF
Weighted Pred (P)                   OFF
Weighted Bipred (B)                 OFF
Direct Prediction                   NO
Direct 8x8 Inference                OFF
SEI                                 NO
VUI                                 NO
Number Slice Groups                 1
Long-term Ref Frames                NO
MMCO                                NO
Arbitrary Slice Order               NO
Redundant Slices                    No

############  Changing Parameters ################
Num. of ref-frames                  4
IDR                                 every 2 Intra
Constrained intra                   OFF
Non-reference frame use             NO
Access unit delimiter               OFF
